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	АННОТАЦИЯ:

	 
	В статье рассмотрены исследования по нанесению никель-фосфорного покрытия на поверхности поршней компрессоров высокого давления из алюминиевых сплавов и предварительной финишной обработки под покрытие. Выбраны параметры, влияющие на скорость осаждения никель-фосфорного сплава и режимы обработки поверхности детали под покрытие. Проведено планирование эксперимента, которое дало возможность отработать оптимальные режимы осаждения и состав покрытия для получения основных высоких показателей качества его поверхности - шероховатости и износостойкости. Проведены экспериментальные исследования по износостойкости образцов с никель-фосфорным покрытием и без покрытия. Целью статьи является технологическое обеспечение износостойкости поршней из алюмининевых сплавов при их восстановлении и эксплуатации в производственных условиях. В работе использованы основные положения технологии химического нанесения покрытия и технологии машиностроения.
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	ОПИСАНИЕ НА АНГЛИЙСКОМ ЯЗЫКЕ:

	 
	INVESTIGATION OF PROPERTIES OF CHEMICAL NICKEL COATINGS DURING RESTORATION OF COMPRESSOR PISTONS MADE OF ALUMINUM ALLOYS, BASED ON APPLICATION OF REGRESSION ANALYSIS
SKRYABIN V.A.1

1 Penza State University, 440026, Russian Federation

	 
	The studies on the deposition of a nickel-phosphorus coating on the surface of high-pressure compressor pistons made of aluminum alloys and the pre-finishing treatment for coating are discussed. The parameters affecting the deposition rate of the nickel-phosphorus alloy and the modes of the surface treatment of a part for coating have been selected. The experiment planning was carried out, which made it possible to work out the optimal deposition modes and the coating composition to obtain the main high quality indicators of its surface, namely roughness and wear resistance. Experimental studies on the wear resistance of samples with the nickel-phosphorus coating and without one were performed. The purpose of the work was to provide technological supply of wear resistance of aluminum alloy pistons during their restoration and operation under production conditions. The main provisions of chemical coating deposition technology and mechanical engineering technology were used.
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